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1. OBJECT AND EXTENT

These guidelines shall secure personnel working in laboratories against accidents and health damages, and that chemical laboratory work at the University of Tromsø (UiTø) are carried out in a safe way and in accordance with laws and directions.  These guidelines apply to all employees, students and guest scientists, working or performing experiments with FLUOHYDRIC ACID in laboratories at UiTø or in buildings that UiTø manage.

2. RESPONSIBILITY

In accordance with the set of rules in Working Environment Act, especially §114, the acting leader or the course supervisor is responsible for: 

· Preparing the conditions in such a way that these guidelines can be complied with.

· That employees and students are familiar with the fact that this work could be dangerous or injurious to health, and that they receive training, practice and the instructions necessary.

· Training http://www.adm.uit.no/persavd/hms/labsikkerhet/index.htm
· That necessary protective equipment are present and are used

Employees and students are responsible for:

· Follow the existing guidelines

· Use necessary protective equipment

· Report to the acting leader or the course supervisor leader any defects or mistakes made 

3. DEFINITIONS

	Acting leader:
	Acting leader: Employee that is appointed to lead or control other employees

	Course supervisor:
	Course supervisor for student’s laboratory courses, and also the teaching supervisor on these courses

	Employee:
	All that has a work relationship to the UiTø (including externally financed), guest scientists and students that in project are connected to a research laboratory.

	Student:
	Registered student at UiTø




4. REFERANSER  OG VEDLEGG

Referanse 1: HMS datablad, VWR International AS 04/09/1998

 Retningslinjer for arbeid med kjemikalier ved UiTø

http://www.adm.uit.no/persavd/reglementer/retningslinjer/hms/kjemlabretn.htm
Sikkerhet på lab ved UiTø

http://www.adm.uit.no/persavd/hms/labsikkerhet/index.htm
Stoffkartoteket UiTø:

http://stoffer.uit.no/
Avfallsrutiner

http://www.adm.uit.no/persavd/reglementer/retningslinjer/hms/spavfall98.htm
Arbeidstilsynets lovdata kap.VII og VIII: 

http://www.lovdata.no/cgi-wift/wiftldles?doc=/usr/www/lovdata/for/sf/aa/aa-20010430-0443.html&dep=aad&emne=443&
Kjemikalieforskriften

http://www.lovdata.no/for/sf/aa/xa-20010430-0443.html
Miljøstatus; stofflisten

http://www.mistin.dep.no/Tema/Kjemikalier/stoffliste/stoffliste.asp
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R26, 27, 28 �
Extremely poisonous if inhaled, swallowed or in contact with skin �
�
R35 �
Strongly corrosive�
�



	


		USE:





Pregnant shall not work with concentrated solutions (>1%)


        Read guidance for pregnant and breast-feeding.





Work with fluohydric acid with concentration > 1% shall take place in a closed hood.


 


Use necessary protective equipment such as lab coat, protective goggles and protective gloves (type nitrile). 


 





		WASTE





Fluohydric acid waste with concentration > 10% are to be delivered as special waste grouped 4.


Fluohydric acid waste with concentration <10% are to be delivered as special waste grouped 6.
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