Attachment 2: LIMIT VALUES


(attachment to instructions for disposal of risk-waste)				    Dated: 1.9.97





Classified according to property-based criterias:�
Danger code�
Percent limits/values 1�
�
Extremely flammable


Flammable�
F�
Flash point below or equal to 55 0 C �
�
Oxidizing


R-8�
O�
�
�
Very toxic


R-26, R-27, R-28�
T+�
Total concentration abow or equal to 0,1%�
�
Very toxic


R-39/26, R-39/27, R-39/28�
T+�
Total concentration abow or equal to 10%�
�
Toxic


R-23, R-24, R-25�
T�
Total concentration abow or equal to 3%�
�
Toxic


R-39/23, R-39/24, R-39/25�
T�
Total concentration abow or equal to 10%�
�
Toxic


R-48/23, R-48/24, R-48/25�
T�
Total concentration abow or equal to 10%�
�
Health damaging


R-20, R-21, R-22�
Xn�
Total concentration abow or equal to 25%�
�
Corrosive


R-35�
C�
Total concentration abow or equal to 1%�
�
Corrosive


R-34�
C�
Total concentration abow or equal to 5%�
�
Irritating


R-41�
Xi�
Total concentration abow or equal to 10%�
�
Irritating


R-36, R-37, R-38�
Xi�
Total concentration abow or equal to 20%�
�
Causing allergy


R-42/43�
Xn/Xi�
Concentration abow or equal to 1%�
�
Causing cancer


(K1) 2, R-45, R-49�
T�
Concentration abow or equal to 0.01%�
�
Causing cancer


(K2), R-45, R-49�
T�
Concentration abow or equal to 0,1%�
�
Causing cancer


(K3), R-215�
Xn�
Concentration abow or equal to 1%�
�
Causing genetic damages


R-46 (kat 1 eller 2)�
T�
Concentration abow or equal to 0,1%�
�
Causing genetic damages


R-40, (kat 3)�
Xn�
Concentration abow or equal to 1%�
�
Causes reproductive damages


R-60, R-61 (kat 1 eller 2)�
T�
Concentration abow or equal to 0,1%�
�
Causes reproductive damages


R-62, R-63�
Xn�
Concentration abow or equal to 5%


�
�
Causes environemtal damages


R-50 - R-59�
ev N�
Percent limits do not exist for mixtures�
�
1: Below these risk levels, the substance may be handeled/destructed by the user; see also # 4.1 in instructions for the management of risk waste.


2: See directions for marking of healt risks, chapt. 4                                                                   H: AKO/Retn/Sp.avfall





