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FORMÅL OG OMFANG

Målet med denne instruksen er å legge til rette for en trygg arbeidsplass for de som arbeider med åpne radioaktive kilder og deres kollegaer. Instruksen gjelder for alle som har behov for  å bruke disse 

Adresse: http://www.fm.uit.no/info/imb/hms/pages/straalevern.html
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1. OBJECT AND EXTENT

These guidelines shall secure personnel working in laboratories against accidents and health damages, and that chemical laboratory work at the University of Tromsø (UiTø) are carried out in a safe way and in accordance with laws and directions.  These guidelines apply to all employees, students and guest scientists, transporting chemicals, special waste, gasses and liquid nitrogen on public roads.

2. RESPONSIBILITY

In accordance with the set of rules in Working Environment Act, especially §114, the acting leader or the course supervisor is responsible for: 

· Preparing the conditions in such a way that these guidelines can be complied with.

· That employees and students are familiar with the fact that this work could be dangerous or injurious to health, and that they receive training, practice and the instructions necessary.

· Training http://www.adm.uit.no/persavd/hms/labsikkerhet/index.htm
· That necessary protective equipment are present and are used

Employees and students are responsible for:

· Follow the existing guidelines

· Use necessary protective equipment

· Report to the acting leader or the course supervisor leader any defects or mistakes made 

3. DEFINITIONS

	Acting leader:
	Acting leader: Employee that is appointed to lead or control other employees

	Course supervisor:
	Course supervisor for student’s laboratory courses, and also the teaching supervisor on these courses

	Employee:
	All that has a work relationship to the UiTø (including externally financed), guest scientists and students that in project are connected to a research laboratory.

	Student:
	Registered student at UiTø



	Dangerous goods
	Dangerous goods are products defined as dangerous goods in accordance with the regulations in ADR and RID.


4. GENERALLY

Dangerous goods are products defined as dangerous goods in accordance with the regulations in ADR and RID. Examples are; Gases, liquid nitrogen, organic solvents, most chemicals and radioactive material.

Use necessary protective equipment and prepare first aid measures.

Bruk alltid nødvendig verneutstyr og sett deg inn i  / klargjør førstehjelpstiltak .

Rapporter farlige situasjoner / uhell ved utfylling av skademeldingsskjema

http://www.fm.uit.no/info/imb/hms/documents/Skadeskjema_210202-1.doc
5. REFERANSER  OG VEDLEGG

ADR / RID
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NOTE:





Hazardous goods are goods that are defined in accordance to the regulations in ADR and RID (Forskrift om landtransport av farlig gods)





Examples of hazardous goods at the UiTø are: 


Gasses, liquid nitrogen, organic solvents, most chemicals and radioactive material (both purchased material and waste).





Transport of hazardous goods on public roads shall always take place in one of the University vehicle(not private cars).





Always see to:





Necessary packaging, labelling and securing of the things about to be transported. 
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