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1. OBJECT AND EXTENT

These guidelines shall secure personnel working in laboratories against accidents and health damages, and that chemical laboratory work at the University of Tromsø (UiTø) are carried out in a safe way and in accordance with laws and directions.  These guidelines apply to all employees, students and guest scientists, working or performing experiments with CARCINOGENIC CHEMICALS in laboratories at UiTø or in buildings that UiTø manage.

2. RESPONSIBILITY

In accordance with the set of rules in Working Environment Act, especially §114, the acting leader or the course supervisor is responsible for: 

· Preparing the conditions in such a way that these guidelines can be complied with.

· That employees and students are familiar with the fact that this work could be dangerous or injurious to health, and that they receive training, practice and the instructions necessary.

· Training Personalkompetanse - HMS
· That necessary protective equipment are present and are used

Employees and students are responsible for:

· Following the existing guidelines

· Using necessary protective equipment

· Reporting to the acting leader or the course supervisor leader any defects or mistakes made 

3. DEFINITIONS

	Acting leader:
	Acting leader: Employee that is appointed to lead or control other employees

	Course supervisor:
	Course supervisor for student’s laboratory courses, and also the teaching supervisor on these courses

	Employee:
	All that has a work relationship to the UiTø (including externally financed), guest scientists and students that in project are connected to a research laboratory.

	Student:
	Registered student at UiTø


4. SUPPLEMENTARY INFORMATION

UiTø keeps an overview over all employees that are in contact with carcinogenic chemicals in their working time.  Stoffkartoteket offer reports over the carcinogenic chemicals in use at UiTø, and where these are stored.

Before you start working with chemicals, read the material safety data sheet.  If the substance is labelled toxic (T), very toxic(T+) or the  Andreascross (Xn) read the risk-sentences carefully!! R-sentence number R40,R44 and R49 say that the substance can be or is carcinogenic. When possible, substitute carcinogenic chemicals for other, none carcinogenic chemicals.

Before you start up working with carcinogenic chemicals, read the MSDS, to be found I nthe chemical database (stoffkartoteket). Especially important are point 3 (Hazards Identification), point 4 (First Aid Measures) and point 8 (Exposure Controls, Personal Protection).  Use necessary protective equipment and prepare first aid measures.

 

Report dangerous situations / accidents by filling out the proper forms found at http://uit.no/getfile.php?PageID=5886&FileId=37

5. LINKS

Stoffkartoteket ved UiTø/HMS datablad – Chemical database at UiTø

Stoffkartoteket Search for relevant chemical
Stofflisten – Dangerous Chemical List

Miljøstatus i Norge Search on: stofflisten

Kjemikalieforskriften – Cheical Regulations

Lovdata Search on: kjemikalieforskriften

Arbeidstilsynet – Labour Inspection

Arbeidstilsynet Search on: HMS datablad
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R45 �
Can cause cancer. �
�
R49�
Can cause cancer if inhaled.�
�
R40�
Limited evidence of a carcinogenic effect�
�



	NOTE


Replace if possible, carcinogenic chemicals with other chemicals.





Read the material safety data sheet (MSDS) before you start using new chemicals. 					 





	PAY SPECIAL ATTENTION TO:


A register shall be kept over personnel that are in contact with carcinogenic chemicals during work (kjemikalieforskriften).





Pregnant and breast-feeding shall be extremely careful, and have the opportunity to select not to work with substances that can cause cancer (See work routine for pregnant and breast feeding).





Handling carcinogenic chemicals in powder form shall take place at an outlet with a closed ventilation system (safety closet).





Handling of concentrated carcinogenic solutions (many organic solvents) shall take place in a closed hood. 





	WASTE:


Waste that exceeds limit value shall be disposed of as special waste. 


(See � HYPERLINK "http://uit.no/hms/5885/1" ��HMS ved UiTø� lover og retningslinjer> retningslinjer > specsialavfall, especially attachment 2) 
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